
Calling from command line for timed record function (all versions):

SAQrxV094_48k.exe [-i] [-o] -txx,yy

Parameters:
       -i : Input  Record (Radio Frequency, samplerate=FS), or -b for stereo input.
       -o : Output Record (Audio Frequency, samplerate= 11.025 or 12kHz)
       xx : Number of minutes to wait for recording after program start
       yy : Number of minutes as duration of recording session                        
       
After start, select manually frequency and filter, then wait ...

-------------------------------------------------------------------
       
Example, best packed in a batchfile timer.bat in the exe directory :
SAQrxV094_192k.exe -i -o -t290,5 

Meaning:
After 290 min of program starting, record both input(RF) and output(audio)
for 5 min duration. 
Now if the program is running, select the desired frequency,filter,level,
then you can do other work. 
Check that the computer do not fall into sleep mode !



      
       